# ProSoft EIP-61850 Configuration Manager 2.0.2.17 Read Me

ProSoft EIP-61850 Configuration Manager 2.0.2.17
ReadMe File

This ReadMe file contains information you should know before you install ProSoft EIP-61850 Configuration Manager version 2.0.2.17. This file also contains information that may not be available in other ProSoft Technology documentation. Visit our website for the most current information about ProSoft EIP-61850 Configuration Manager.

Version 2.0.2.17 Changes:

Fixed an issue with configuration manager crash when comments were included within the DA (Data Attribute) section of the .cid file.

# ProSoft EIP-61850 Configuration Manager Compatibility

The following system requirements apply to ProSoft EIP-61850 Configuration Manager.

ProSoft EIP-61850 Configuration Manager installation instructions are provided in the ProLinx PLX8x-EIP-61850 user manual.

> Note: System requirements in this document are subject to change and do not represent a commitment to support any particular software or hardware.

## ProSoft EIP-61850 Configuration Manager Operating Systems Tested

- Windows 7 Professional (32-bit and 64-bit versions), 8 GB RAM Intel® Core™ i5 650 (3.20 GHz)
- Windows XP Professional Ver.2002 Service Pack 2, 512 MB RAM Pentium 4 (2.66 Gz)

> NOTE: To use ProSoft EIP-61850 Configuration Manager under the Windows 7 OS, you must be sure to install ProSoft EIP-61850 Configuration Manager using the Run as Administrator option. To find this option, right-click on the Setup.exe installer program icon. In the context menu, you will see the Run as Administrator option. Left-click to use this install option. Be aware, you must install using this option even if you are already logged in as an Administrator on your network or personal computer (PC). Using the Run as Administrator option will allow the ProSoft EIP-61850 Configuration Manager installer to create folders and files on your PC with proper permissions and security. If you do not use the Run as Administrator option, ProSoft EIP-61850 Configuration Manager may appear to install correctly; but you will receive numerous, repeating file access errors whenever ProSoft EIP-61850 Configuration Manager is running, especially when changing configuration screens. If this happens, to eliminate the errors, you will have to completely uninstall ProSoft EIP-61850 Configuration Manager and then re-install using the Run as Administrator option.

# Previously Released versions of ProSoft EIP-61850 Configuration Manager

ProSoft EIP-61850 Configuration Manager 2.0.2.16

Detailed Reason(s) for Version 2.0.2.16 Changes:

Fixed an issue with configuration manager crash when comments were included within the DO (Data Object) section of the .cid file.

ProSoft EIP-61850 Configuration Manager 2.0.2.15

Detailed Reason(s) for Version 2.0.2.15 Changes:

Fixed an issue where the proper .dll files were not included with the installer file.

ProSoft EIP-61850 Configuration Manager 2.0.2.10

Detailed Reason(s) for Version 2.0.2.10 Changes:

Added support to the PLX82-EIP-61850 Dual and Single Ethernet Port functionalities. Fixes issue with CIDs whose first five characters of the name are equal. Fixes issue with exporting AOIs.

ProSoft EIP-61850 Configuration Manager 1.0.7.1

Detailed Reason(s) for Version 1.0.7.1 Changes:

Fixes uploading issue where the configuration file was uploaded using a new computer.

ProSoft EIP-61850 Configuration Manager 1.0.6.1

Detailed Reason(s) for Version 1.0.6.1 Changes:

Fixes issues related to the exporting of gi parameter,and the tag name truncating.

ProSoft EIP-61850 Configuration Manager 1.0.4.7

Detailed Reason(s) for Version 1.0.4.7 Changes:

Supports SBO and enhanced security control; fixes compatibility issues with Areva CID files, numeric suffix were removed from default tag name.

ProSoft EIP-61850 Configuration Manager 1.0.0.96

Detailed Reason(s) for Version 1.0.0.96 Changes:

Initial Release.